|  |  |  |
| --- | --- | --- |
| **DEC** | **HEX** | **ERROR CODE** |
|  |  | **COMX 35 Error Message** |
| 0 | 0 | Program halted by user |
| 1 | 1 | Syntax error in asc or len function |
| 2 | 2 | Array out of range or not dimensioned |
| 3 | 3 | Dimension error |
| 4 | 4 | Defint has illegal ending |
| 5 | 5 | Parentheses missing in argument |
| 6 | 6 | Argument out of range |
| 7 | 7 | Mixed mode calculation encountered |
| 8 | 8 | Divide by zero error, or log of negative number |
| 9 | 9 | Non-executable function encountered |
| 10 | A | Exit command must be used with for/next or gosub/return |
| 11 | B | For/next stack overflow, or for/next executed directly |
| 12 | C | Syntax error in for |
| 13 | D | Gosub stack overflow |
| 14 | E | Unacceptable character in hexadecimal number |
| 15 | F | Floating point number too large to be converted to integer or integer multiply overflow |
| 16 | 10 | Unacceptable operator in conditional statement |
| 17 | 11 | Input or fval cannot be directly executed |
| 18 | 12 | Must have variable or string name in read |
| 19 | 13 | Syntax error in read or input |
| 20 | 14 | Syntax error in len function |
| 21 | 15 | Syntax error in assignment statement |
| 22 | 16 | Missing quote |
| 23 | 17 | Syntax error in list |
| 24 | 18 | No such word found in library |
| 25 | 19 | Syntax error in mid$ function |
| 26 | 1A | Unacceptable variable name found in next statement |
| 27 | 1B | Either a number or a letter is expected |
| 28 | 1C | Missing arithmetic parentheses |
| 29 | 1D | Wrong number of arguments in poke statement |
| 30 | 1E | Unacceptable last character in print statement |
| 31 | 1F | Syntax error in data statement |
| 32 | 20 | No more data found |
| 33 | 21 | No such string found in input statement |
| 34 | 22 | Missing equal sign in assignment statement |
| 35 | 23 | Missing parentheses in string array |
| 36 | 24 | Too many arguments in usr or call |
| 37 | 25 | Syntax error in chr$ function |
| 38 | 26 | Unacceptable character in binary number |
| 39 | 27 | Line buffer overflow |
| 40 | 28 | File not opened for input |
| 41 | 29 | File not opened for output |
| 42 | 2A | Unacceptable line end or non-executable statement |
| 43 | 2B | Stack overflow |
| 44 | 2C | Too many digits in number |
| 45 | 2D | Unacceptable character in number fold |
| 46 | 2E | No such line number found |
| 47 | 2F | Unacceptable operation in if statement |
| 48 | 30 | Memory overflow |
| 49 | 31 | Wrong number of arguments in mod statement |
| 50 | 32 | Program too large for memory |
| 51 | 33 | Argument out of range |
| 52 | 34 | Wrong number of arguments |
| 53 | 35 | Wrong number of arguments |
| 54 | 36 | String variable not defined |
| 55 | 37 | Tape read error |
| 56 | 38 | Tape write error |
| 57 | 39 | File is not a basic program |
| 58 | 3A | File is not basic data |
| 59 | 3B | Reserved |
| 60 | 3C | Reserved |
| 61 | 3D | Reserved |
| 62 | 3E | Rom or rom card not present |
| 63 | 3F | Not enough memory for renumber to operate |
| 64 | 40 | Renumber located line number error |
| 65 | 41 | No such subscript variable defined |
| 66 | 42 | String is over 127 characters |
| 67 | 43 | Number of arguments in color must be 1 |
| 68 | 44 | Number of arguments in screen must be 1 |
| 69 | 45 | Number of arguments in ctone must be 1 |
| 70 | 46 | Number of arguments in volume must be 1 |
| 71 | 47 | Number of arguments in noise must be 2 |
| 72 | 48 | Number of arguments in tone or music must be 3 |
|  |  | **F&M BASIC V2.00 ERROR MESSAGES (1/2)** |
| 73 | 49 | Number of arguments in TEXT must be 1 |
| 74 | 4A | Number of arguments in POINT must be 2 |
| 75 | 4B | Number of arguments in DUMP must be 2 |
| 76 | 4C | Number of arguments in CHAR must be 1 |
| 77 | 4D | Incorrect use of ALPHA |
| 78 | 4E | Line number missing |
| 79 | 4F | TOS not found |
|  |  | **PRINTER ERROR** |
| 80 | 50 | Printer error |
|  |  | **F&M BASIC V2.00 ERROR MESSAGES (2/2)** |
| 81 | 51 | Number of arguments in P-SCR must be 1 |
| 82 | 52 | Not enough memory for P-SCR |
| 83 | 53 | Number of arguments in DEL must be 1 or 2 |
| 84 | 54 | First argument in DEL must be lower than last |
| 85 | 55 | TOS command not recognized |
|  |  | **SB ERROR MESSAGES** |
| 86 | 56 | Only one parameter (B, I, R, T) allowed |
| 87 | 57 | Invalid parameter |
| 88 | 58 | Program will not fit into 8K RAM bank |
| 89 | 59 | Number of arguments in USB MOVE must be 3, 4 or 6 |
| 90 | 5A | Syntax error in CARD statement |
| 91 | 5B | No rtc or nvram found, or nvram not initiated |
| 92 | 5C | No valid data in RAM bank |
| 93 | 5D | Could not delete file |
| 94 | 5E | No data to save |
| 95 | 5F | No disk card or disk not initiated |
| 96 | 60 | Too many parameters |
| 97 | 61 | Nvram write enable error |
| 98 | 62 | Specify date string |
| 99 | 63 | Incorrect date string format |
| 138 | 8A | Incorrect I/O port specified |
| 139 | 8B | Number of arguments in USB OUT must be 2 |
| 140 | 8C | Number of arguments in USB PPOKE or USB NVPOKE must be 2 |
| 141 | 8D | NVPOKE or NVSTART address out of nvram range |
| 142 | 8E | USB command not recognized |
| 143 | 8F | Help for command not found |
| 144 | 90 | Command ROM not detected |
| 145 | 91 | Unknown or incorrect file format |
| 146 | 92 | F&M BASIC not loaded |
| 147 | 93 | File name too long |
| 148 | 94 | No filename specified |
| 149 | 95 | Address range required |
| 150 | 96 | End address required |
| 151 | 97 | Invalid RAM bank |
| 152 | 98 | Invalid directory |
| 153 | 99 | Could not create directory |
| 154 | 9A | Specify start < end address |
| 155 | 9B | Could not delete directory |
| 156 | 9C | Specify start address |
| 157 | 9D | Incorrect line number |
| 158 | 9E | Number of arguments in USB CPOS must be 2 |
| 159 | 9F | Specify start <= DEFUS address |
| 160 | A0 | Program cannot be loaded in F&M BASIC |
| 161 | A1 | Number of arguments in USB NVPUT must be 3 |
| 162 | A2 | NVRAM full, data not stored |
| 163 | A3 | Software ID not found |
| 164 | A4 | Number of arguments in USB NVGET must be 2 |
| 165 | A5 | Number of arguments in USB NVIGET , NVSGET, NVDEL and NVSTART must be 1 |
| 166 | A6 | Requested NVRAM size to small to fit current data |
| 167 | A7 | Software ID should be between 1 and 255 |
| 168 | A8 | Label or date string too long |
| 169 | A9 | No label or date string specified |
| 170 | AA | No or incorrect printer card found |
| 171 | AB | Printer not on |
| 172 | AC | Number of arguments in USB MEMDUMP and USB PMEMDUMP must be 3 |
| 173 | AD | Wrong disk format, image is single sided/ single density |
| 174 | AE | Wrong disk format, image is single sided/double density |
| 175 | AF | Wrong disk format, image is double sided/single density |
| 176 | B0 | Incorrect EF flag specified |
| 177 | B1 | 80 column card not found |
| 178 | B2 | RAM bank file not found |
| 179 | B3 | USB transfer timeout |
| 180 | B4 | USB transfer error |
| 181 | B5 | Two file names required |
| 182 | B6 | Card type not found |
| 183 | B7 | Network error |
| 184 | B8 | Online features disabled |
| 185 | B9 | Server error |
| 186 | BA | URL not found |
| 187 | BB | Number of arguments in USB PLOT must be 3 or 4 |
| 188 | BC | Number of arguments in USB LINE or USB ELLIPSE must be 5 |
| 189 | BD | Number of arguments in USB CIRCLE must be 4 |
| 190 | BE | Number of arguments in USB CPEEK must be 1 or 2 |
| 191 | BF | No REM statement found |
| 192 | C0 | Number of arguments in USB CPOKE must be 2 or 3 |
|  |  | **COMX 35 DOS ERROR MESSAGE** |
| 100 | 64 | Text file record length is not fixed |
| 101 | 65 | Record number exceeds file size |
| 102 | 66 | Disk read error |
| 103 | 67 | Read or write pointer exceeds file size |
| 104 | 68 | Sector read or write error |
| 105 | 69 | Seek error |
| 106 | 6A | Diskette write protected |
| 107 | 6B | File locked |
| 108 | 6C | Spare |
| 109 | 6D | Spare |
| 110 | 6E | Slash missing |
| 111 | 6F | End of command found |
| 112 | 70 | Work id. Number error |
| 113 | 71 | Record length missing |
| 114 | 72 | More than 8 arrays already exist |
| 115 | 73 | String or array variable error |
| 116 | 74 | Not integer or too large integer exist |
| 117 | 75 | Not a fixed record length file type |
| 118 | 76 | String exceeds record length |
| 119 | 77 | Spare |
| 120 | 78 | Address syntax error |
| 121 | 79 | Drive number argument or syntax wrong |
| 122 | 7A | Not enough disk memory |
| 123 | 7B | Parenthesis missing |
| 124 | 7C | Input file name error |
| 125 | 7D | Comma missing |
| 126 | 7E | Command does not exist |
| 127 | 7F | Syntax error on ‘save’ command |
| 128 | 80 | Quotation mark missing |
| 129 | 81 | File name already opened or exists in directory |
| 130 | 82 | File not found in directory |
| 131 | 83 | No such kind of protection |
| 132 | 84 | More than 5 files already opened |
| 133 | 85 | File name not yet opened |
| 134 | 86 | More than 51 directory entries |
| 135 | 87 | File write protected |
| 136 | 88 | Disk or file non-copyable |
| 137 | 89 | No such handler command code |